|  |  |  |
| --- | --- | --- |
| **1. Product/Substance Detail** | | **Hazard symbol** |
| Name of substance / product: | **Emulsion** |  |
| Supplier / manufacturer: |  |
| Form of substance: | Liquid |
| Substance used for / product of: | Painting |

|  |  |
| --- | --- |
| **2. Health Hazards, Treatment and Protection** | |
| **If inhaled** | |
| First-Aid: | Remove to fresh air, keep patient warm and at rest. If breathing is irregular or stopped administer artificial respiration. Give  nothing by mouth. If unconscious place in the recovery position. Seek medical advice. |
| Control measures required: |  |
| **If ingested** | |
| First-Aid: | If accidentally swallowed, DO NOT INDUCE VOMITING. Keep at rest and obtain medical attention. |
| Control measures required: |  |
| **Contact with skin** | |
| Effect: |  |
| First-Aid: | Remove contaminated clothing, wash skin thoroughly with soap and water, or use a proprietary skin cleanser. Do not use  solvents or thinners. Seek medical advice if symptoms persist. |
| Control measures required: |  |
| **Contact with eyes** | |
| Effect: |  |
| First-Aid: | Remove contact lenses. Irrigate copiously with clean, fresh water for at least 10 minutes, holding lids apart. Seek medical advice. |
| Control measures required: |  |

|  |  |
| --- | --- |
| **3. Storage and Handling** | |
| Storage: | Observe the label precautions. Store in a cool, dry, well ventilated place away from sources of heat, ignition and  direct sunlight. No smoking. Prevent unauthorised access. Containers which are opened should be properly resealed and kept upright to prevent  leakage. Do not use or store any paint container by hanging on a hook. |
| Handling: | Prevent air-borne concentrations higher than the occupational exposure limits. Keep the container tightly closed.  Exclude sources of heat, sparks and open flame. Avoid skin and eye contact. Avoid inhalation of vapour. Smoking, eating and drinking should be prohibited in storage and use areas Always keep in containers made of the same material as the supply container, or in containers that are compatible with the product. |

|  |  |
| --- | --- |
| **4. SPILLAGE AND DISPOSAL** | |
| Spillage: |  |
| Disposal: | Do not empty into drains or watercourses. |

|  |  |
| --- | --- |
| **5. FIRE SAFETY** | |
| Fire Extinguisher type: | Recommended - alcohol resistant foam, CO2, powders. Do not use water jet |

|  |  |
| --- | --- |
| **6. General** | |
| General Precautions: | Ensure area to be used is well ventilated with through flow of air.  Ensure workers take regular breaks away from the painting area  Eating or drinking not to be carried out in the painting area  Gloves offered if required |

**Produced By:** …J Lediard **Date:** July 2011

**This sheet must be stored in the same place as the chemical.**