|  |  |
| --- | --- |
| **1. Product/Substance Detail** | **Hazard symbol** |
| Name of substance / product: | **White Spirit** |  |
| Supplier / manufacturer: |  |
| Form of substance: | Liquid |
| Substance used for / product of: | Cleaning painting equipment |

|  |
| --- |
| **2. Health Hazards, Treatment and Protection** |
| **If inhaled** |
| Effect: | Irritating to respiratory system. |
| First-Aid: | Move the exposed person to fresh air at once. Get medical attention. |
| Control measures required: | Use in well ventilated area. If ventilation is insufficient wear breathing protection |
| **If ingested** |
| Effect: | Irritating. May be absorbed in the body and cause dizziness, nausea and vomiting. Diarrhoea. |
| First-Aid: | Provide rest, warmth and fresh air. Immediately rinse mouth and drink plenty of water (200-300 ml). Get medical attention. |
| Control measures required: |  |
| **Contact with skin** |
| Effect: | Irritating to skin. |
| First-Aid: | Remove contaminated clothing immediately and wash skin with soap and water. Get medical attention immediately. |
| Control measures required: | Gloves are recommended |
| **Contact with eyes** |
| Effect: | Irritating and may cause redness and pain. |
| First-Aid: | Immediately flush with plenty of water for up to 15 minutes. Remove any contact lenses and open eyes wide apart. Get medicalattention immediately. Continue to rinse. |
| Control measures required: | Wear approved safety goggles. |

|  |
| --- |
| **3. Storage and Handling** |
| Storage: | Keep containers tightly closed. Keep in original container. Keep away from heat, sparks and open flame. |
| Handling: | Avoid spilling, skin and eye contact. Keep away from heat, sparks and open flame. Eliminate all sources of ignition. Providegood ventilation. Avoid inhalation of vapours and spray mists. |

|  |
| --- |
| **4. SPILLAGE AND DISPOSAL** |
| Spillage: |  |
| Disposal: | Waste to be treated as controlled waste. Disposal to licensed waste disposal site in accordance with local Waste DisposalAuthority. Do not puncture or incinerate even when empty. Rags and the like, moistened with flammable liquids, must be discarded into designated fireproof bucket.Dispose of waste and residues in accordance with local authority requirements. |

|  |
| --- |
| **5. FIRE SAFETY** |
| Fire Extinguisher type: | Extinguish with alcohol-resistant foam, carbon dioxide, dry powder or water fog. |

|  |
| --- |
| **6. General** |
| General Precautions: |  |

 **Produced By:** …J Lediard **Date:**

**This sheet must be stored in the same place as the chemical.**